**
**
**  VIA PCI Card Reader Host Controller
**
**  WDM Driver for Windows 2000/XP/Svr2003/Vista x86 edition
**
**  v1.44   Jul, 2009
**
**

Introduction:
=============

  This document shows you how to setup the driver in Windows operating system.

Contents of the Subdirectory:
=============================

    VIACR.SYS            The WDM x86 driver for Windows 2000/XP/Svr2003/Vista.
    VIACR.INF            The installation information file.
    VIACR.CAT            The WDM x86 driver Windows logo signature file.
    CRICON.DLL           The customized memory card drive icons dll file.
    VIACR.TXT            This file.

Installation:
=============

  Before starting with the installation process, make sure that the adapter
  is properly installed and configured.

    1. Turn on the power of your PC to boot into Windows operating system.
       Windows will auto-detect your new hardware, and the "New Hardware Found"
       dialogue box will appear. Select "Driver from disk provided by hardware
       manufacturer" to install driver from the driver diskette or other location.

    2. When the driver installation is completed, restart Windows if needed.

