Release Notes for ACR38U SAM drivers:
=====================================

----------------------------------------------------
Update: 1.0.2.6 (RW)	      Date: 02-December-2009
----------------------------------------------------

Description:
- ACS ACR38U-SAM driver package for win98/ME, 2000, XP, 2003/2008, Vista and Windows 7 (x86 & x64).

Changes:
- WHQL certified drivers signed by Microsoft for:
  * 2000
  * Windows XP (x86 & x64)
  * Windows Vista (x86 & x64)
  * Windows 7 (x86 & x64)
  * Windows Server 2003 (x86 & x64)
  * Windows Server 2008 (x86 & x64)
  * Windows Server 2008 R2 (x64)

----------------------------------------------------
Version: 1.0.2.6 (RW)	      Date: 03-November-2009
----------------------------------------------------

Description:
- ACS ACR38U-SAM driver package for win98/ME, 2000, XP, 2003/2008, Vista and Windows 7 (x86 & x64).

Changes:
- Fixed driver load/unload problems in Windows 7.
- Fixed memory problems found with WHQL Driver Verifier Test.
- Fixed memory problem found with WHQL Plug and Play Driver Test.
- Fixed problems found with WHQL Device Path Exerciser Test.
- Fixed problem found with WHQL Pnpdtest with concurrent IO in parallel with DevPathExer.
- Fixed sleep-mode handling.
- Renamed service name to prevent conflict with ACR38U in Win98.
- Updated inf-file.
- ACS SPC Signed for Vista/Win7 x86 & x64.

----------------------------------------------------
Version: 1.0.2.5 (RW)		Date: 29-August-2007
----------------------------------------------------

Description:
- Released to ACS (Windows 98, windows 2000/XP and Vista x86 & x64)

Changes:
- Based on IRIS 1.0.2.8 driver
- INF-file updated
  - include x64 OS.
  - increased USB timeout to 120 seconds (solved timeout in ACOS5 RSA key generation)

Known issues:
- On FW 1.04s: has synchronisation issues with Axalto 32K eGate highspeed card (WHQL card)

----------------------------------------------------