                     

 	   USB Tool for Windows 98/ME/2000/XP

  		   Release 1.00
	ConTouch TouchSystems Technology Co., Ltd.

The USB Tool for Windows 98/ME/2000/XP contains a 
HID (Human Interface Device) filter driver designed 
for Windows using the WDM (Windows Driver Model) 
architecture, setup program, video alignment program,
uninstall utility, and 32-bit control panel for ConTouch
TouchSystems TouchMonitors and controllers.

=======================================================
Supported Touchscreen Controllers
=======================================================

   - ConTouch USB Controllers (CA-20U)

==============================
CONTENTS
==============================

1.Install/Uninstall Manual
  1.1 Installing touchscreen driver for Windows 98/ME/2000/XP
  1.2 Change touchscreen settings
  1.3 Uninstall touchscreen software
  1.4 Release Notes	
2.Problem solution

========================================
1.	Install/Uninstall Manual
========================================

1.1 Installing touchscreen driver for Windows 98/ME/2000/XP

Note to Windows 2000 users: you must have administrator access rights on your 
Windows 2000/XP system to install this software for Windows 98/ME/2000/XP. 
You must also have administrator access rights to run the touchscreen control 
panel and video alignment programs.

Shutdown your computer and connect your touchmonitor as described
in the accompanying documentation.

A. Install standard HID mouse driver for our touchscreen
------------------------------------------------------------

=========
NOTES:
=========

If you have installed our USB interface touchscreen before,you can simply skip this 
installation stage.

   1. Windows find our touchscreen,recognize it as a standard HID device,and prompt you
      to install driver for it.
	      	
   2. Choose "Next". Select "Search for the best driver for
      your device (Recommended)" and Choose "Next".

   3. Install the standard HID mouse driver for our touchscreen,
      Wait while driver files are copied to your computer. Insert
      your Windows CD if prompted. After successful installation,
      You may notice that a touch will move the Windows cursor even 
      before you begin the second installation stage marked as B.

B. Install our updated touchscreen driver and utilities
-------------------------------------------------------------

   1. Click the "Start" button, and then click "Run".

   2. Click the "Browse" button to locate the "Setup.exe" program on
      the floppy drive containing this software for Windows disk.
      Insert the disk into your floppy drive. (If the driver
      files have been copied to your hard drive or have been
      distributed on CD, use "Browse" to select the directory
      containing the driver files.)

      Highlight Setup.exe and click "Open", then "OK" to run
      Setup.exe.

   3. Follow the directions on the screen.

   4. If the "Digital Signature Not Found" dialog is displayed by
      Windows, click "Yes" to continue the installation. This
      version of touchscreen driver for Windows has not yet been tested by
      Microsoft.

   5. Restart Windows when prompted. Make sure you remove any
      floppy disks. 

      The touchscreen video alignment program will automatically
      run when Windows starts up. Touch each of the three targets
      as they appear on the screen. Click "Yes" when the cursor
      lines up correctly with your finger.

=========================================
1.2	Change Touchscreen settings
=========================================

1. Click the "Start" button, point to "Settings", and then click
   "Control Panel".

2. Double-click the "ConTouch Touchscreen" icon,now you can change 
   your touchscreen settings.

=========================================
1.3 	Uninstalling touchscreen driver for Windows 98/ME/2000/XP
=========================================

1. Click the "Start" button, point to "Settings", and then click
   "Control Panel".

2. Double-click the "Add/Remove" Programs icon.

3. Select "ConTouch TouchSystems USB Tools" from the list of
   uninstallable programs on the "Install/Uninstall" tab.

4. Click the "Add/Remove" button then follow the directions on
   your screen.

===============================
1.4	Release Notes
===============================

=================
HID Class Devices
=================

- Because your ConTouch Touchscreen USB controller conforms 
  to the USB HID class specification, Windows 98/ME/2000/XP supports 
  it inherently with default HID class drivers. You may notice that 
  a touch will move the Windows cursor even before you install 
  this device driver package for Windows.

  However, you must install this driver package in order to install 
  and use the video alignment program (used to correctly align your 
  finger to the Windows cursor) and our control panel.

- Windows 2000 only: you must have administrator access rights to
  run the ConTouch Touchscreen control panel and video alignment
  programs.

==============================
2.	Problem solution
==============================

-  If you never install our USB touchscreen before and when you first 
   plug our touchscreen USB cable,Windows will recognize it as a standard 
   HID mouse,you can install a standard HID mouse driver for it and then 
   run Setup.exe program to install our touchscreen driver.

-  A touch will not wake the system when in Stand-by power save
   mode. Move the mouse or press a key on the keyboard to return
   from Stand-by mode. Disable Stand-by mode in the Power
   Management control panel to avoid this issue when the USB
   touchscreen is your only input device.

