 Elo XP Universal Driver for Windows XP and Windows 2000

                       Release 4.40 
                      March 23, 2006
                     Elo TouchSystems
         A Division of Tyco Electronics Corporation


Elo XP Universal Driver contains native 32-bit drivers designed 
for Windows XP and Windows 2000, a setup program, video alignment 
program, control panel program, tool tray application and right 
button application for Elo TouchSystems' touchmonitors.  

=======================================================
Supported Touchmonitors and Elo Touchscreen Controllers
=======================================================

   - All Elo Entuitive brand touchmonitors with a USB
     controller

   - Elo USB Controllers (IntelliTouch(R) 2216, 2600, 2500U,
     2700, 2701, AccuTouch(R) 3000U, CarrollTouch(R) 4000U, 
     4500U, Surface Capacitive 5000)

   - All Elo Entuitive brand touchmonitors with an internal
     serial controller

   - Elo Serial Controllers (IntelliTouch(R) 2500S, 2310B, 
     2216, 2310, 2300, 2700, 2701, AccuTouch(R) 2210, 
     CarrollTouch(R), 4000S, 4500S, Surface Capacitive 5000)

   --------------------------------------------------------
  |                                                        |
  | This driver does not support Elo PC-Bus controllers.   |
  |                                                        |
  | Refer to www.elotouch.com for availability of drivers  |
  | for these products.                                    |
  |                                                        |
   --------------------------------------------------------

===============================================================
Installing Elo XP Universal Driver Windows XP or Windows 2000
===============================================================

Note: you must have administrator access rights on your 
Windows XP or Windows 2000 system to install Elo XP Universial 
Driver for Windows. 

Shutdown your computer and connect your touchmonitor as described
in the accompanying documentation. Restart your computer.

Windows 2000 and XP Installation:
---------------------------------

Browse to the directory containing the driver installation 
package files. 

Double click on EloSetup.exe to run the install application.

=================================================================
Uninstalling Elo XP Universal Driver Windows XP or Windows 2000 
=================================================================

1. After Windows loads, click the Start button, click Settings, 
   and then click Control Panel. 

2. Double-click the Add/Remove Programs icon.

3. Select Elo XP Universal Driver from the list of
   uninstallable programs on the Install/Uninstall tab.

4. Click the Add/Remove button then follow the directions on
   your screen.

=============
Release Notes
=============

- A touch may not wake the system when in Stand-by power save
  mode. Move the mouse or press a key on the keyboard to return
  from Stand-by mode. Disable Stand-by mode in the Power
  Management control panel to avoid this issue when the USB
  touchscreen is your only input device.

- Full Screen DOS sessions are not supported. However, windowed
  DOS mode is fully supported. A touch to a full-screen DOS
  session will cause your system to immediately return to your
  Windows desktop. A mouse can be used to access programs run
  in a Full Screen DOS session.

==============
Contacting Elo
==============

www.elotouch.com

e-mail: eloinfo@elotouch.com

Elo TouchSystems
A Division of Tyco Electronics Corporation
301 Constitution Drive
Menlo Park, CA 94025
USA
Phone: (800) 557-1458
       (650) 361-4700
Fax:   (650) 361-4747

Elo TouchSystems GmbH & Co. KG
Haidgraben 6
D-85521 Ottobrunn
Germany
Phone: +49 (0) 89/60822-0
Fax:   +49 (0) 89/60822-150

Elo TouchSystems, NV
Diestsesteenweg 692
B-3010 Kessel-Lo
Belgium
Phone: +32 (16) 35-2100
Fax:   +32 (16) 35-2101

Copyright (c) 2006 Elo TouchSystems
All rights reserved.

