IE SmartReader - PCSC/CCID Driver Release Information
====================+++++++++++++++==================

Version No.	Date		Changes
1.1.0.5		13 nov 2006	The Power Management problem solved;
						FW update problem fixed.

1.1.0.4		11 oct 2006	The internal request and the reply buffers are extended.

1.1.0.3		18 may 2006	The PCSC Device name is now derived from the USB EEPROM configuration.

1.1.0.2		14 mar 2006	Request data len fixed;
						Rx and Tx Timeout setting fixed.

1.1.0.1		28 apr 2005	IOCTL commands fixed for Share Direct mode.

1.1.0.0		21 mar 2005	IOCTL commands added;
						Default RxTimeout changed from 1 to 5 sec,
						as solution to cards initialization.

1.0.0.2		20 jan 2005	Registry Debug Params added;
						Reader state SCARD_SWALLOWED replaced by SCARD_POWERED
						on card insersion;
						Inf file updated for install/uninstall procedure.

1.0.0.1		29 dec 2004	Filter function added. The reader can also be controled
						by the FTDI FTD2XX.DLL functions.

1.0.0.0		20 dec 2004	Initial PCSC/CCID Version.

