This folder contains USB drivers for the Allen-Bradley 1203-USB product. 
Plug the 1203-USB into a USB port on your computer. You should then
get a new hardware found message. When you are requested to supply 
the source of these drivers, specify this directory. Follow the directions.
These drivers will create a virtual COM port on your computer. 
Find the port number from the Ports (COM & LPT) portion of your computer's hardware device manager.
Set the baud rate for this port to 115.2KB in DriveExplorer or RSLinx and connect as usual.  
More explicit directions are in the file "USB Driver Installation Instructions.doc" in this directory.





