
       USB Tool for Windows XP and Windows 2000

                     Release 2.30
                   November 12, 2001
                 Elo TouchSystems, Inc.

The USB Tool for Windows XP and Windows 2000 contains a 
HID (Human Interface Device) filter driver designed for 
Windows using the WDM (Windows Driver Model) architecture, 
setup program, video alignment program, uninstall utility, 
and 32-bit control panel program for Elo TouchSystems' USB 
touchmonitors and USB touchscreen controllers.

=======================================================
Supported Touchmonitors and Elo Touchscreen Controllers
=======================================================

   - All Elo Entuitive brand touchmonitors with a USB
     controller

   - Elo USB Controllers (IntelliTouch(R) 2600, 2500U,
     AccuTouch(R) 3000U)

   --------------------------------------------------------
  |                                                        |
  | This driver does not support Elo serial Touchmonitors, |
  | Elo serial controllers or Elo PC-Bus controllers.      |
  |                                                        |
  | Refer to www.elotouch.com for availability of drivers  |
  | for these products.                                    |
  |                                                        |
   --------------------------------------------------------

===================================================
Installing USB Tool for Windows XP or Windows 2000
===================================================

Note to Windows XP and Windows 2000 users: you must have 
administrator access rights on your Windows XP or Windows 2000 
system to install USB Tool for Windows. You must also have 
administrator access rights to run the touchscreen control 
panel and video alignment applications.

Shutdown your computer and connect your touchmonitor as described
in the accompanying documentation.

A. If Windows STARTS the New Hardware Wizard
--------------======------------------------

   1. Choose Next. Select "Search for the best driver for
      your device (Recommended)" and Choose Next.

   2. When a list of search locations is displayed, place a
      checkmark on the floppy drive containing this USB Tool
      for Windows disk. Insert the disk into your floppy drive.
      (If the driver files have been copied to your hard drive or
      have been distributed on CD, place a checkmark on "Specify
      a location" and use Browse to select the directory
      containing the driver files.)

   3. Choose Next. Once the Elo TouchSystems USB Touchmonitor
      Interface driver has been detected choose Next again.

   4. Wait while driver files are copied to your computer. Insert
      your Windows CD if prompted.

   5. Choose Finish. 

B. If Windows DOES NOT START the New Hardware Wizard
--------------==============------------------------
 
   1. After Windows loads, click the Start button, and then 
      click Control Panel, System, Device Manager. 

   2. In the Device Manager, right click on the USB Human 
      Interface Device, and then click on Properties, Driver 
      tab, Update Driver, Next. Select "Search for the best driver 
      for your device (Recommended)" and Choose Next.

   3. When a list of search locations is displayed, place a
      checkmark on the floppy drive or CD containing this USB Tool
      for Windows disk. Insert the disk into your drive. (If the 
      driver files have been copied to your hard drive, place a
      checkmark on "Specify a location" and use Browse to select 
      the directory containing the driver files.)

   4. Choose Next. Once the Elo TouchSystems USB Touchmonitor
      Interface driver has been detected choose Next again.

   5. Wait while driver files are copied to your computer. Insert
      your Windows CD if prompted.

   6. Choose Finish. 

   7. The alignment application, Elova.exe, must be used 
      manually to align cursor movement with point of touch.


====================================================
Uninstalling USB Tool for Windows XP or Windows 2000 
====================================================

1. Click the Start button, point to Settings, and then click
   Control Panel.

2. Double-click the Add/Remove Programs icon.

3. Select Elo USB Tool for Windows from the list of
   uninstallable programs on the Install/Uninstall tab.

4. Click the Add/Remove button then follow the directions on
   your screen.

5. Restart Windows to complete the uninstall process.

7. The alignment application, Elova.exe, must be used 
   manually to align cursor movement with point of touch.


=================
HID Class Devices
=================

Because your Elo USB touchmonitor or touchscreen controller
conforms to the USB HID class specification, Windows XP and 
Windows 2000 support it inherently with default HID class 
drivers. You may notice that a touch will move the Windows 
cursor even before you install this USB Tool for Windows.

However, you must install the USB Tool for Windows in order to
install and use the video alignment application (used to
correctly align your finger to the Windows cursor) and Elo
control panel.

=============
Release Notes
=============

- You must have administrator access rights to run the 
  Elo Touchscreen control panel and video alignment
  applications.

- The control panel and video alignment applications will report
  errors with one or more drivers if the 2.0 or 3.0 release of Elo
  MonitorMouse serial touch interface drivers are loaded along
  with the Elo USB Tool for Windows. These serial drivers do not
  have the appropriate version data to function with these 
  applications. You can avoid these error messages by uninstalling 
  the serial drivers.

- A touch will not wake the system when in Stand-by power save
  mode. Move the mouse or press a key on the keyboard to return
  from Stand-by mode. Disable Stand-by mode in the Power
  Management control panel to avoid this issue when the USB
  touchscreen is your only input device.

- Full Screen DOS sessions are not supported. However, windowed
  DOS mode is fully supported. A touch to a full-screen DOS
  session will cause your system to immediately return to your
  Windows desktop. A mouse can be used to access programs run
  in a Full Screen DOS session.

==========================================
Enhancements and Bug Fixes in This Release
==========================================

- Added support for display size larger than touchscreen.

==========
Known Bugs
==========

- The touchscreen will not work properly when the mouse is
  set for left-handed button configuration in the Mouse
  Properties control panel. Touch will always perform a right
  mouse function when the mouse is set for a left-handed
  user.

- If you press the Cancel button on the Elo Touchscreen
  control panel after using the Apply button, some of the
  applied settings will become un-applied.

- Uninstalling the driver will leave the following benign
  empty folder on your hard drive:

   C:\Program Files\Elotouch

==============
Contacting Elo
==============

www.elotouch.com

e-mail: eloinfo@elotouch.com

Elo TouchSystems, Inc.
6500 Kaiser Drive
Fremont, CA 94555
USA
Phone: (800) 557-1458
       (510) 739-4999
Fax:   (510) 739-5353

Elo TouchSystems GmbH & Co. KG
Haidgraben 6
D-85521 Ottobrunn
Germany
Phone: +49 (0) 89/60822-0
Fax:   +49 (0) 89/60822-150

Elo TouchSystems, NV
Diestsesteenweg 692
B-3010 Kessel-Lo
Belgium
Phone: +32 (16) 35-2100
Fax:   +32 (16) 35-2101

Copyright (c) 2000 Elo TouchSystems, Inc.
All rights reserved.
